Main

GET Value on IR in

IF IR Pin High

STOP Listening on RF Module

START Writing on RF Module

SEND Unit ID

START Listening

START Unit LED

BEGIN LED’s timer

IF Radio message available

COLLECT Entirety of message

START Message’s LED

BEGIN LED’s timer

LED Timers

IF LED’s timer is greater than defined interval

Turn LED OFF

ELSE

Keep LED ON